For 1990-2009 cars

### Removal Procedure

1. Using a small flat-bladed tool release the pressure clip at the leading edge of the side marker lamp housing between the headlamp and the fender.
2. Remove the side marker lamp housing by pulling the leading edge forward and straight out.
3. Rotate the side marker lamp bulb socket counter clockwise ¼ turn.

Pull the socket rearward until the bulb clears the side marker lamp housing assembly.

4. Remove the bulb from the bulb socket.

### Installation Procedure

1. Install the bulb to the bulb socket,
2. Position the side marker lamp socket into the side marker lamp.

Rotate the side marker lamp socket clockwise ¼ turn to lock in place.

3. Insert the tab at the back of the side marker lamp into the fender pressing into place until fully seated.