For 1990-2009 cars

### Removal Procedure

1. Pull on the rear seat cushion retainer strap while pulling up on the cushion to disengage the forward attachment. of the rear seat cushion
2. Push the cushion rearward to disengage the rear attachment. Lift the cushion out of the vehicle while carefully routing the seat belts through the cushion opening.

### Installation Procedure

1. Position the seat cushion over the rear seat floor area.
2. Route the rear seat belts through the cushion openings.
3. Slide the seat cushion frame into the rear attaching brackets.
4. Push downward at the seat cushion forward retainers to lock the cushion to the floor brackets.