For 1990-2009 cars

### Removal Procedure

1. Remove the upper steering column trim cover and lower the steering column cover fasteners.
2. Remove the ignition switch bezel and remove the lower cover.
3. Remove the park lock solenoid electrical connector.
4. Remove the park lock solenoid screws and remove the park lock solenoid from the vehicle.

### Installation Procedure

1. Position the park lock solenoid onto the column and install the screws.

Tighten
Tighten the park lock solenoid screws to 1.5 Nm (14 lb in).

2. Connect the park lock solenoid electrical connector.
3. Install the lower steering column trim cover and the ignition switch bezel.
4. Install the lower steering column trim cover fasteners.

Tighten
Tighten the steering column trim cover attaching fasteners to 4 Nm (35 lb in).

5. Install the upper steering column trim cover.