For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Jam/Ajar Switch to Body Fasteners | 2.0 N·m | 18 lb in
Glove Compartment Bin to I/P Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Door Fasteners | 2 N·m | 18 lb in
Ignition Switch Fasteners | 1.5 N·m | 13 lb in
Latch Assembly Retaining Bolts | 10 N·m | 89 lb in
Lock Cylinder Actuator to Latch Assembly Screws | 10 N·m | 89 lb in
Lock Cylinder Assembly Retaining Nuts | 3.0 N·m | 27 lb in
Lower Rear Window Guide Bolt | 10 N·m | 89 lb in
Park Lock Solenoid Screws | 1.5 N·m | 14 lb in
Power Door Lock Screws | 10 N·m | 89 lb in
Rear Window Run channel Bolts | 10 N·m | 89 lb in
Steering Column Trim Cover Attaching Fasteners | 4 N·m | 35 lb in
Steering Wheel Shroud Fasteners | 3 N·m | 27 lb in