For 1990-2009 cars

### Removal Procedure

1. Remove rear transaxle mount through bolt.
2. Remove one of three transaxle mount bracket to frame bolts.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

3. Raise vehicle on hoist.
4. Remove remaining mount bracket to frame attachment bolts.
5. Remove transaxle mount bracket from vehicle.
6. Remove the transaxle mount to transaxle bolts.
7. Remove transaxle mount from vehicle.

### Installation Procedure

1. Install rear transaxle mount to transaxle and tighten fasteners.

Tighten
Tighten Rear Transaxle Mount-to-Transaxle Bolts to: 90 N·m (66 lb ft)

2. Install the two transaxle mount bracket to frame attachment fasteners and tighten.

Tighten
Tighten Rear Transaxle Mount Bracket-to-Frame Bolts to: 60 N·m (44 lb ft)

3. Lower vehicle from hoist.
4. Install and tighten the transaxle mount bracket to frame attachment fastener.

Tighten
Tighten Rear Transaxle Mount Bracket-to-Frame Bolts to: 60 N·m (44 lb ft)

5. Install the transaxle mount to bracket through bolt.

Tighten
Tighten Rear Transaxle Mount Through Bolt to: 90 N·m (66 lb ft)