For 1990-2009 cars

#### Tools Required

• | 87 92 210 Differential Bearing Support

• | SA9120T Differential Bearing Installer

• | SA9172G Ball Detent Handle

• | SA9211T-2 5th Gear Puller

• | SA9211T2-4 Thread On Adapter

### Disassembly Procedure

1. Mount the differential in a vise with soft jaws.

Notice: The thread on adapter must be used on the 5th gear puller when removing the differential bearings. If the adapter is not used, the puller can be damaged.

2. Remove the differential bearings using the SA9211T-2 with the SA9211T2-4 . Use the 87 92 210 as a base for the puller as shown.