For 1990-2009 cars

Table 1: | Scan Tool Only Content Theft Programming

### RKE Customer Programmable Content Theft Programming

To enter programming mode:

1. Press the PANIC button on the transmitter 8-10 times in 5 seconds with the ignition ON.
2. Within 3 seconds, select the mode by pressing LOCK, UNLOCK, or TRUNK button.

• | Active -- The content theft system will only be armed by using the transmitter to lock the doors.

• | Passive -- The content theft system will arm 5 minutes after the ignition is OFF, all the doors and the trunk are closed. Any door open will reset 5 minute timer.

• | Disabled -- No content theft system activated.

Press to Select Mode | Mode Selected | Description | Feedback
--- | --- | --- | ---
Press UNLOCK | Disabled | Content theft system disabled | BCM chime once upon receipt of transmitter feedback
Press LOCK | Active | Content theft system active upon RKE LOCK command and IGN OFF, all the doors and the trunk closed | BCM chime once upon receipt of transmitter feedback
Press TRUNK | Passive | System will arm 5 minutes after the vehicle is secured | BCM chime once upon receipt of transmitter feedback

#### Scan Tool Only Content Theft Programming

Mode | Description | Feedback | Default State
--- | --- | --- | ---
Pre-alarm 0 | Content theft system feedback before full alarm | Chirp horn for 10 seconds | Disabled
Pre-alarm 1 | Content theft system feedback before full alarm | BCM chime for 10 seconds | Enabled
Pre-alarm 2 | Content theft system feedback before full alarm | Silent | Disabled
Pre-alarm 3 | Content theft system feedback before full alarm | No pre-alarm | Disabled
Arming 1 | Content theft system status | RKE arming only | Enabled
Arming 2 | Content theft system status | RKE and passive arming | Disabled
Arming 3 | Content theft system status | Content theft system disabled | Disabled