For 1990-2009 cars

### Fusible Link

• | Inspect link for damage or discoloration

• | Test for battery voltage on both ends of link

• | Replace with same size fusible link (wire-gauge size printed on insulation)

### Ignition Switch Continuity

Important: Key-minder circuit is open until ignition switch is cycled.

### Neutral Safety Backup Switch (NSBU)

1. Disconnect neutral safety backup switch (NSBU).
2. Using DVOM, check for continuity between terminals G and E on the NSBU switch when vehicle is in Park or Neutral position.

### Clutch Start Switch (Manual)

1. Disconnect clutch start switch electrical connector.
2. Use a fused jumper wire to bypass switch by connecting terminal A to terminal B.

Important: Switch is faulty if engine cranks normal.