For 1990-2009 cars

#### Tools Required

J 43654 Piston Pin Clip Remover and Installer

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

1. Disassemble the piston rings. Use a suitable tool in order to expand the rings. The piston rings must not be reused.

Important: Two retainers hold the piston pins in place. No special tools are required to remove the retainers or the piston pins. Ensure that the piston pin is not damaged. Do not reuse the retaining clips.

2. Remove the piston pin retaining clips using the J 43654 .
3. Remove the piston pin.

#### Tools Required

J 43654 Piston Pin Clip Installer

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

1. Disassemble the piston rings. Use a suitable tool in order to expand the rings. Piston rings must not be reused.
2. Remove the piston pin retaining clips using the J 43654 .
3. Remove the piston pin.