For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Oil in Compressor (A/C System) | 220 ml PAG | 7.5 oz PAG
Oil Quantities needed due to part replacement

- Evaporator
- Condenser
- Receiver/Dehydrator

- 72 ml
- 38 ml
- 11 ml

- 2.4 oz
- 1.3 oz
- 0.4 oz

Large Leak | 132 ml | 4.5 oz
R134a Refrigerant Change | 0.950 kg | 2.0 lb + 1.5 oz
Compressor Displacement | 9-140 cc | --
High Pressure Relief Valve

- Opens
- Reseat

- 3260 + 345/-245 kPa
- 2930 kPa

- 525 psi
- 425 psi

Compressor Clutch Gap | 0.3-0.6 mm | 0.012-0.024 in
Coolant Volumes (Dex-Cool™)

- L81
- L61

- 7.4 L
- 7.0 L

- 7.8 qt
- 7.4 qt