For 1990-2009 cars

# Front Brake Rotor Minimum Thickness After Refinish and Discard Thickness Specifications

Subject: | Information on Front Brake Rotor Minimum Thickness After Refinish and Discard Thickness Specifications

Models: | 2000-2002 Saturn L-Series Vehicles

### Condition

The purpose of this bulletin is to provide revised front brake rotor specifications and to update all 2000/2001 and 2002 L-Series Brakes Service Manuals.

Please obtain all 2000/2001 L-Series Brakes Service Manuals at your location and update as indicated.

Revised Front Brake Rotors Specifications
-- | mm | in
Minimum Thickness After Refinish | 22.3 | 0.878
Discard Thickness | 22.0 | 0.866
Minimum After Turning | 22.3 | 0.878
Discard | 22.0 | 0.866

1. In the 2000/2001 L-Series Brakes Service Manual:

• | On page 11, under front brake rotors, cross out the specifications values for Brake Rotors Minimum Thickness After Refinish and Discard Thickness and write in the values from the table above.

• | On page 67, in Front Rotor Thickness Chart, cross out the specifications values for Minimum After Turning and Discard and write in values from the table on the previous page.

2. In the 2002 L-Series Brakes Service Manual:

• | On page 19, under Front Brake Rotors, cross out the specifications values for Brake Rotors Minimum Thickness After Refinish and Discard Thickness and write in the values from the table on the previous page.

• | On page 77, in Front Rotor Thickness Chart, cross out the specifications values for Minimum After Turning and Discard and write in the values from the table on the previous page.