For 1990-2009 cars

## Rear Split Folding Seat Back Replacement Sedan

### Removal Procedure

Important: The rear seat back attachments have an Easyload™ outer bracket that allows the rear seat back to snap into position upon installation. It is necessary to gently pry the Easyload bracket outward to remove the rear seat back. It is important not use excessive force to pry on the bracket or the bracket may become damaged. Move the bracket only enough to lift the seat back from the vehicle. If the bracket has been moved outward too much, gently reposition the bracket to ensure proper retention of the rear seat back to the bracket.

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. With your hand, push on the seat back foam to expose the seat bracket outer retainer.
3. Unlatch the seat back. Leave the seat in the upward position.
4. Using a flat-bladed tool gently pry the outer seat bracket retainer inward while pulling upward on the seat back to disengage the outer bracket from the pivot pin.
5. Remove the seat back.

### Installation Procedure

1. Guide the seat back assembly onto the center pivot pin. Ensure that the seat back locates into the inner pivot tabs.
2. Align the outer pivot pin with the lead in the ramp on the Easyload bracket.
3. Push downward on the seat back to engage the Easyload bracket.
4. Raise the seat backs and secure the seat back latch.
5. Install the seat cushion. Refer to Rear Seat Cushion Replacement .

## Rear Split Folding Seat Back Replacement Wagon

### Removal Procedure

Important: The rear seat back attachments have an Easyload outer bracket that allows the rear seat back to snap into position upon installation. It is necessary to gently pry the Easyload bracket outward to remove the rear seat back. It is important not use excessive force to pry on the bracket or the bracket may become damaged. Move the bracket only enough to lift the seat back from the vehicle. If the bracket has been moved outward too much, gently reposition the bracket to ensure proper retention of the rear seat back to the bracket.

#### Driver Side

1. Lower the passenger side rear seat back to the full down position.
2. Unlatch the rear seat back. Leave the seat in the upward position.
3. With your hand, push on the seat back foam to expose the seat bracket outer retainer.
4. Using a flat-bladed screwdriver gently pry the outer seat bracket retainer inward while pulling upward on the seat back, to disengage the outer bracket from the pivot pin.
5. Lift the seat back up and remove it from the vehicle.

#### Passenger Side

1. With your hand, push on the seat back foam to expose the seat bracket outer retainer.
2. Unlatch the rear seat back. Leave the seat in the upward position.
3. Using a flat-bladed screwdriver gently pry the outer seat bracket retainer inward while pulling upward on the seat back, to disengage outer bracket from the pivot pin.
4. Tilt the seat back down to align the inner pivot tabs, then pull the seat back outward to remove the seat back.

### Installation Procedure

1. Guide the seat back assembly onto the center pivot pin. Ensure that the seat back locates into the inner pivot tabs.
2. Align the outer pivot pin with the lead in the ramp on the Easyload bracket.
3. Push downward on the seat back to engage the Easyload bracket.
4. Raise the seat backs and secure the seat back latch.