For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate pull handle plugs.
2. Remove the fasteners and the liftgate pull handle.
3. Remove the liftgate trim panel retainers.
4. Remove the trim panel.

### Installation Procedure

1. Position the liftgate trim panel to the liftgate.
2. Secure to the structure by pushing at the retainer locations.
3. Install the trim panel retainers.
4. Install the liftgate pull handle using the fasteners.

Tighten
Tighten the liftgate inner pull handle fasteners to 5 N·m (44 in lb)

5. Install the liftgate pull handle plugs.