For 1990-2009 cars

#### Tools Required

• | J 41228 Stub Shaft Sleeve Installer

• | SA9211T 5th Gear Remover

### Removal Procedure

1. Remove the transaxle case side cover. Refer to Control Valve Body Cover Replacement .
2. Remove the snap ring from the output axle shaft and discard.
3. Remove the output axle shaft sleeve from the output shaft using SA9211T .

### Installation Procedure

1. Use J 41228 to install new sleeve on output axle shaft. Ensure that collet is located in snap ring groove when installing.
2. Install a new snap ring on output axle shaft.
3. Install the transaxle case side cover. Refer to Control Valve Body Cover Replacement .
4. Start engine, warm up transaxle, and check for leaks.
5. Inspect the fluid level. Refer to Transmission Fluid Check Procedure.