For 1990-2009 cars

### Removal Procedure

1. Disable the SIR System. Refer to SIR Disable/Enable Procedure.
2. Position the steering column to its lowest position.
3. Remove the I/P cluster trim plate. Refer to I/P Cluster Trim Plate.
4. Remove the upper and lower cluster fasteners and pull rearward to remove the I/P cluster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the I/P cluster into the I/P housing ensuring that the cluster harness is connected. Install and tighten the fasteners.

Tighten
Tighten the I/P cluster trim plate-to-I/P housing fasteners to 2.5 N·m (22 lb in).

2. Install the I/P cluster trim plate. Refer to I/P Cluster Trim Plate.
3. Enable the SIR System. Refer to SIR Disable/Enable Procedure.