For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Battery Hold-Down Bracket | 20 N·m | 15 lb ft
Battery Hold Down Bracket Bolt | 20 N·m | 15 lb ft
Battery Terminal Bolts | 17 N·m | 13 lb ft
Belt Tensioner Bolts | 40 N·m | 30 lb ft
Condenser Block-to-Radiator End Tank Bolt | 4 N·m | 35 lb in
Condenser-to-Radiator Bolts | 4 N·m | 35 lb in
Degas Pipe-to-Head Bolt | 10 N·m | 89 lb in
Fan Shroud-to-Radiator Bolts | 4 N·m | 35 lb in
Front Timing Belt Cover Bolt | 8 N·m | 71 lb in
Intake Manifold Bolt | 20 N·m | 15 lb ft
Left Headlamp Assembly Bolts | 10 N·m | 89 lb in
Liquid Line Clamp-to-Condenser Bolt | 4 N·m | 35 lb in
Lower Cradle Splash Shield Fasteners | 5 N·m | 44 lb in
Lower Fan Shroud-to-Condenser Bolts | 4 N·m | 35 lb in
Lower Fan Shroud-to-Condenser Mounting Studs | 4 N·m | 35 lb in
Lower Transaxle Cooler Line-to-Radiator End Tank | 4 N·m | 35 lb in
Lower Transmission Cooler Line-to-Radiator End Tank | 25 N·m | 18 lb ft
Power Steering Fluid Reservoir-to-Fan Shroud Bolts | 5 N·m | 44 lb in
Puller Fan Shroud-to-Radiator Bolts | 4 N·m | 35 lb in
Radiator Bracket-to-Rail Bolts | 6 N·m | 53 lb in
Splash Shield Bolts | 5 N·m | 44 lb in
Thermostat Housing Bolts | 20 N·m | 15 lb ft
Thermostat Housing-to-Block Bolts | 10 N·m | 89 lb in
Upper Transaxle Cooler Line-to-Radiator End Tank | 25 N·m | 18 lb ft
Upper Transmission Cooler Line-to-Radiator End Tank | 25 N·m | 18 lb ft
Water Pump Bolts | 25 N·m | 18 lb ft
Water Pump Mount and Heat Shield Block Bolt | 8 N·m | 71 lb in
Water Pump Pulley Bolt | 8 N·m | 71 lb in
Water Pump Sprocket-to-Water Pump Bolts | 10 N·m | 89 lb in