For 1990-2009 cars

### Removal Procedure

1. Remove the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement .
2. Remove the nuts attaching the fog lamp bracket to the impact bar.
3. Remove the fog lamp assembly and bracket down through the bottom of the front fascia.
4. Remove the fog lamp assembly from the fog lamp bracket.

### Installation Procedure

1. Install the fog lamp assembly to the fog lamp bracket.
2. Place the fog lamp assembly and bracket into position through the bottom of the front fascia.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the 2 nuts attaching the fog lamp bracket to the impact bar.

Tighten
Tighten the fog lamp bracket-to-impact bar fasteners to 30 N·m (22 lb ft).

4. Install the headlamp housing. Refer to Headlamp Assembly or Headlamp Bulb Replacement .