For 1990-2009 cars

#### Tools Required

• | J 41239-10 Cooler Line Seal Removal

• | J 45201 Cooler Line Seal Removal

Important: If you have special tool J 41239-10 use step 1 and 2 only.

1. Install J 41239-10 between the cooler line seal (49) and the case.
2. It may be necessary to pivot J 41239-10 back and forth against the case to remove the seal.

Important: If you have special tool J 45201 use step 3 - 6 only.

3. Insert J 45201 collet (2) fully into the cooler line seal bore.
4. Insert the forcing screw piece of the J 45201 (1) into J 45201 (2) and tighten.
5. Thread the J 45201 collar (2) onto J 45201 (3) and tighten until the tool has removed the seal.
6. Use a pair of pliers to remove the cooler line seal from J 45201 .