For 1990-2009 cars

### Removal Procedure

1. Gently pry at the rear of the sunroof switch to release the clips.
2. Slightly rotate the switch while removing to allow room for the electrical connector.
3. Remove the switch from the opening.
4. Disconnect the electrical connector from the switch.

### Installation Procedure

1. Connect the electrical connector to the switch.
2. Rotate the switch into the opening and press into place until fully seated.
3. Cycle the sunroof to verify proper operation.