For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Pull back the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the bolts from the window run channel.
4. Remove the foam insinuator pad.
5. Remove the weatherstrip from the window run channel.

### Installation Procedure

1. Install the weatherstrip to the window run channel.
2. Position the window run channel to the rear door.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the window run channel bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the foam insulator pad.
5. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
6. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .