For 1990-2009 cars

### Removal Procedure

Important: On vehicles with L61 engines and cruise control, it is necessary to remove the left stabilizer bar clamp with the vehicle on a hoist.

1. Remove the stabilizer bar clamps.
2. Remove the bushing from the stabilizer bar.

### Installation Procedure

Important: The opening in the stabilizer bar bushing must face toward the front of the vehicle.

1. Install new stabilizer bar bushings.
2. Install the stabilizer bar clamps and tighten.

Tighten
Tighten the stabilizer bar clamp-to-frame bolts to 20 N·m (15 lb ft).