For 1990-2009 cars

#### Tools Required

• | 83 90 114 Sleeve

• | 83 90 312 Drift, Bearing Race Input Shaft

• | 87 91 220 Drift, Main Shift Rod Bushing

• | 87 91 311 Sleeve, Bearing Driver Shaft

• | 87 92 210 Support, Differential Bearing

• | 87 92 236 Support

• | SA91113T Axle Seal Installer

• | SA9172G Ball Detent Handle

1. Press in the new differential bearing race using the SA9113T and the SA9172G . Use the 87 92 236 as a base for the pressing operation.
2. Install the new axle using the SA9113T and SA9172G .
3. Install the shift control shaft bushing until flush with the inside of the case using the 87 91 220 .
4. Fill the shift control shaft seal lips with grease and drive into the clutch housing using the 87 92 210 and a hammer. The spring side of the seal should face in.
5. Press in the new input shaft bearing race using the 83 90 312 . Use the 83 90 114 and the 87 91 311 as a base for the pressing operation.