For 1990-2009 cars

### Removal Procedure

#### Tools Required

SA9150BR Engine Support Fixture

1. Remove battery from vehicle. Refer to Battery Removal Procedure
2. Remove Underhood Fuse Block (UHFB). Refer to UHFB Removal Procedure
3. Remove battery tray.
4. Install Engine Support Fixture SA9150BR and J43450 Engine Support Fixture Adapter. (L61 engine)
5. Install engine support fixture SA9150E (or equivalent) and J43450 (or equivalent). (L81 engine)
6. Remove transaxle mount to bracket bolts.
7. Remove transaxle mount to body fasteners.
8. Remove transaxle mount from vehicle.

Important: The automatic and manual transaxle mount brackets are different. The following two steps show each.

9. Remove transaxle mount bracket to transaxle fasteners. (Manual)

### Disassembly

Remove bracket from transaxle mount.

### Assembly

Install bracket onto transaxle mount and tighten.

Tighten
Tighten Left Transaxle Mount Bracket-to-Transaxle Mount Bolt to: 60 N·m (44 lb ft)

### Installation Procedure

Important: The automatic and manual transaxle mount brackets are different. The following two steps show each.

1. Install transaxle mount bracket to transaxle. (Manual)

Tighten
Tighten Left Transaxle Mount Bracket-to-Transaxle Bolts (Manual) to: 55 N·m (41 lb ft)

2. Install transaxle mount into vehicle and install mount to body bolts.

Tighten
Tighten Left Transaxle Mount-to-Body Bolts to: 20 N·m (15 lb ft)

3. Install transaxle mount to bracket bolts.

Tighten
Tighten Left Transaxle Mount-to-Transaxle Bracket Bolts to: 55 N·m (41 lb ft)

4. Remove engine support fixture.
5. Install battery tray.

Tighten
Tighten Battery Tray Bolts to: 15 N·m (11 lb ft)

6. Install Underhood Fuse Block (UHFB). Refer to UHFB Installation Procedurer
7. Install battery into vehicle. Refer to Battery Installation Procedure