For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the push-in retainers from the outer edge of the front air deflector to the fascia.
3. Remove the front air deflector from the fascia.

### Installation Procedure

1. Position the lower deflector to the fascia.
2. Install the push-in retainers to the front air deflector to the fascia.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .