For 1990-2009 cars

### Removal Procedure

1. Flip the rear compartment floor carpet away from the side carpet.
2. Remove the rear compartment side carpet fasteners.
3. Remove the side carpet assembly.

### Installation Procedure

1. Position the side carpet to the vehicle.
2. Install the side carpet fasteners.
3. Position the decklid weatherstrip over the rear compartment side carpet.
4. Position the floor carpet into place.