For 1990-2009 cars

### Removal Procedure

1. Ensure the window is in the full-up position.
2. Remove the outer door panel. Refer to Rear Door Outer Panel removal .
3. Remove the door sound deadener at the rear.
4. Remove the lock rod from the latch mechanism.
5. Remove the clip and lock cylinder.

### Installation Procedure

1. Install the lock cylinder and clip.

Important: The lock rod retainers used in the door lock levers and mechanisms are not re-usable. The retention characteristics are minimized once a rod is extracted. The retainers must be replaced every time a rod is extracted.

2. Install the lock rod to the latch mechanism with a new retainer.
3. Install the door sound deadener at the rear.
4. Install the outer door panel. Refer to Rear Door Outer Panel installation procedure .
5. Verify the proper outer door panel fit on all edges, adjacent panels, and to the lock cylinder. Adjust as necessary.
6. Verify the correct and smooth operation.