For 1990-2009 cars

1. Remove the power steering pump, if equipped.
2. Remove the camshaft cover grounding strap.
3. Remove the front lift bracket.
4. Remove the rear lift bracket.
5. Remove the ignition module and coil assembly.
6. Remove the camshaft cover assembly.

### Removal Procedure

1. Remove the power steering pump, if equipped.
2. Remove the camshaft cover grounding strap.
3. Remove the front lift bracket.
4. Remove the rear lift bracket.
5. Remove the ignition module and coil assembly.
6. Remove the camshaft cover assembly.