For 1990-2009 cars

## CD Changer/Player Installation - Retailer Installed Accessory Sedan

### Preparation

Important: Before disconnecting the negative battery cable, make sure that the customer's radio theft deterrent system has been deactivated. If the system is in the SECURE state, refer to theft deterrent feature, to deactivate this feature.

1. Record the preset radio stations.
2. Disconnect the negative battery terminal.

Caution: When you are performing service on or near the SIR components or the SIR wiring, you must disable the SIR system. Refer to Disabling the SIR System. Failure to follow the correct procedure could cause air bag deployment, personal injury, or unnecessary SIR system repairs.

3. Disable the SIR system. Refer to Disabling the SIR System in SIR.

### I/P CD Jumper Installation

1. Open the glove compartment door.
2. Remove the glove compartment lamp assembly by pulling on the lamp plunger.
3. Disconnect the wiring harness connector from the glove compartment lamp.
4. Remove the right side I/P lower closeout, hush panel, retainers.
5. Pull the closeout panel, hush panel, rearward to detach from the forward retainers.
6. Remove the right side heater outlet assembly retainer and remove the outlet.
7. Remove the glove compartment fasteners and the door.
8. Remove the glove compartment bin fasteners.
9. Slowly remove the glove compartment bin and tilt the bin downward to expose the BCM residing on top of the glove compartment.
10. Remove the BCM from the glove compartment by sliding the module out of the attaching slots.
11. Remove the glove compartment bin.
12. Let the BCM hang on the wiring harness.
13. Remove the right hinge pillar molding, kick panel.

13.1. | Remove the upper push pin fastener using a trim panel tool.

13.2. | Remove the fuse box door and pull on the hinge pillar molding at the clip location to disengage the molding.

13.3. | Slide the hinge pillar molding out from under the carpet retainer and remove the hinge pillar molding.

14. Gain access to the rear of the radio and connect the CD I/P harness to the radio.

Important: The I/P harness connector, the antenna connector, and the ground strap terminal do not need to be disconnected, unless the radio needs to be upgraded. Ensure connection.

14.1. | Remove the radio. Refer to Radio Replacement .

14.2. | Upgrade the radio, if necessary, to AM/FM stereo cassette player and CD player with equalizer, UP0.

14.3. | Connect the I/P CD jumper connector to the rear of the radio.

| Important: Do not secure the radio or trim in place until the CD changer/player is installed and verified to be functioning correctly.

14.4. | Set the radio into the radio brace.

15. Route the I/P CD jumper from the rear of the radio to right I/P fuse block.

15.1. | Route the I/P CD jumper behind the right side of the radio to the right of the H-brace, along side of the current routing for the I/P harness.

15.2. | Attach the I/P CD jumper to the I/P lead that connects to the radio using the buddy clip on the harness to hold the jumper in place.

15.3. | Route the I/P CD jumper along the I/P beam and attach the fir tree clips to the vertical side of the beam forward in the car. These clips are located just below the current routing for the I/P harness in the area above the glove compartment bin.

15.4. | Route the I/P CD jumper the rest of the way to the right I/P fuse block area.

### Body CD Jumper Installation

1. Remove the right side of the carpet retainer, sill plate.

1.1. | Move the front seat to the forward most position.

1.2. | Starting at the front of the vehicle, remove the carpet retainer by gently pulling on the retainer at the attaching clip locations.

2. If there are leather seats, move the rear seat cushion forward before removing bolster to avoid damage to the leather.

If the seat is not leather, movement is not necessary.

3. Remove the right rear seat bolster.

3.1. | Reach down into the outer corner of the rear seat cushion to expose the bolster retainer tab.

3.2. | Bend the tab upward.

3.3. | Starting at the bottom, pull forward to disengage the bolster from the retainer tab, then pull upward to disengage the upper attachment.

4. Remove the rear compartment side carpet.

4.1. | Flip the rear compartment floor carpet away from the right side of the vehicle.

4.2. | Remove the rear compartment side carpet fastener as shown.

4.3. | Remove the side carpet assembly.

5. Route the body CD jumper along the right side of the vehicle starting at the area between rear seat and rear compartment.
6. Route the body CD jumper connector through hole found beneath the right rear seat bolster and put enough of the harness through to reach the CD changer/player location.

Notice: Make sure the body CD jumper is lined up correctly with holes before attaching them. The clips are easily damaged when removed.

7. Install the body CD jumper to the vehicle starting with the jumper clip nearest the CD changer/player connector. Attach all of the other clips as you route the body CD jumper to the rear seat area.
8. Route the body CD jumper along the rear seat and install the jumper to the vehicle using attachment clips.
9. Open the harness channel found in the right inner rocker panel area and install the body CD jumper.
10. After installing the harness, close the harness channel.
11. Connect the body CD jumper connector to the I/P CD jumper connector which was routed earlier and is located near the right I/P fuse block (RIPFB) area.
12. Connect the body CD jumper connector to the RIPFB using the rosebud clip on the connector.

### CD Changer/Player Installation

Important: The CD changer/player unit must be installed after the bracket is installed.

Important: If a U-nut is already present at the lower attachment point on the sheet metal, it will be used later in this procedure to install the convenience net.

1. Install the U-nuts to a specified attachment point in the sheet metal.

Important: Do not install the fasteners that attach the trunk side carpet to the vehicle.

2. Position the rear compartment side carpet to the side of the vehicle.
3. Using a sharp knife, carefully cut a hole in raised portion of the rear compartment side carpet at the U-nut location to proved room for the bracket to go through the carpet and attach to vehicle.
4. Align the bracket over the side trim ensuring the bracket is straight.
5. Mark with a pen or sharp tool where the Riv-Nut holes are beneath it.
6. Mark with a pen or sharp tool where the connector should come through, near the lower edge of the bracket.
7. Pull the bracket away.
8. Using a sharp knife, carefully cut holes in the rear compartment side carpet for fasteners to go through into the Riv-Nuts.
9. Pull the body CD jumper through trunk side carpet slit.
10. Position the rear compartment side carpet back in place to side of vehicle.
11. Install the fasteners that attach the rear compartment side carpet to vehicle
12. Position the decklid weather-strip over the rear compartment side carpet.
13. Position the rear compartment floor carpet into place.
14. Hold the bracket in the installation location.

Notice: Refer to Fastener Notice in the Preface section.

15. Attach the bracket to the vehicle with the screws.

Tighten
Tighten the CD changer/player bracket-to-vehicle fastener to 8 N·m (71 lb in).

16. Before fastening the CD changer/player to bracket, make the electrical connection and temporarily connect the negative battery cable. Verify that the CD changer/player is functioning properly, then disconnect the negative battery cable.
17. Install the CD changer/player to bracket.

Tighten
Tighten the CD changer/player-to-CD changer/player bracket fasteners to 4 N·m (35 lb in).

18. If equipped with a convenience net, attach the U-Nut to side attachment on the CD changer/player bracket.
19. Attach the convenience net to the CD changer/player bracket.

### Removed Parts From the Harness Installation

Important: Ensure that the I/P harness connector, antenna connector, and the ground strap connector are connected.

1. Install the radio. Refer to Radio Replacement .
2. Install the glove compartment bin partially into the opening.
3. Secure the BCM to the glove compartment bin slots.
4. Route the glove compartment lamp wiring harness to the lamp opening and connect the wiring harness to the glove compartment lamp.
5. Snap the lamp into the glove compartment bin.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the glove compartment bin to the I/P with fasteners.

Tighten
Tighten the glove compartment bin-to-I/P fasteners to 2.5 N·m (22 lb in).

7. Install the heater outlet with the retainer to glove compartment bin.
8. Install the right lower I/P closeout panel, hush panel, with retainers.
9. Install glove compartment door with fasteners.

Tighten
Tighten the glove compartment door fasteners to 2 N·m (18 lb in).

10. Operate the glove compartment lamp and glove compartment door to assure proper operation.
11. Install the right hinge pillar molding, kick panel.

11.1. | Slide the hinge pillar molding into the carpet retainer.

11.2. | Position the hinge pillar molding to body and install by pushing gently at the clip location.

11.3. | Install the hinge pillar molding upper push pin fastener.

11.4. | Install the fuse box door.

11.5. | Install the weather-strip over the hinge pillar molding cover using a flat blade tool.

12. Install the right side carpet retainer, sill plate.

12.1. | Position the carpet retainer into the vehicle.

12.2. | Starting at the rear of the vehicle, slide the carpet retainer under the rear seat cushion.

12.3. | Position the carpet retainer over the remaining attaching clip locations.

12.4. | Gently push on the attaching clips to install the carpet retainer.

12.5. | Install the weather-strip over the carpet retainer using a flat blade tool.

Caution: Make sure the rear seat shoulder belt is not caught behind the bolster when installing the bolster.

Important: If leather rear seat cushion was removed, install it after installing right rear seat bolster.

13. Install the right rear seat cushion bolster.

13.1. | Position the rear seat bolster onto the upper bolster attachment.

13.2. | Push down on the bolster to engage the upper attachment and install the over retaining tab.

13.3. | Bend the lower retainer tab over the bolster wire frame at the rear seat cushion location.

14. Install the rear compartment side carpet.

• | Install the side carpet assembly.

• | Install the rear compartment side carpet as shown in illustration.

• | Flip the rear compartment floor carpet down toward the right side of the vehicle.

### Remote CD Changer/Player Installation Finishing Touches

1. Enable the SIR System. Refer to Enabling the SIR System in SIR.
2. Connect the negative battery cable.
3. Test the operation of CD Changer/Player. If the CD Changer/Player does not operate correctly, refer to the troubleshooting portion of the audio section.
4. Set earlier recorded radio preset stations and clock time.
5. Remind customer that the Theft Deterrent Feature is not activated and that it needs to be reactivated if continued security is desired.

## CD Changer/Player Installation - Retailer Installed Accessory Wagon

### Preparation

Important: Before disconnecting the negative battery cable, make sure that the customer's radio theft deterrent system has been deactivated. If the system is in the SECURE state, refer to theft deterrent feature, to deactivate this feature.

1. Record the preset radio stations.
2. Disconnect the negative battery terminal.

Caution: When you are performing service on or near the SIR components or the SIR wiring, you must disable the SIR system. Refer to Disabling the SIR System. Failure to follow the correct procedure could cause air bag deployment, personal injury, or unnecessary SIR system repairs.

3. Disable the SIR system. Refer to Disabling the SIR System in SIR.

### I/P CD Jumper Installation

1. Open the glove compartment door.
2. Remove the glove compartment lamp assembly by pulling on the lamp plunger.
3. Disconnect the wiring harness connector from the glove compartment lamp.
4. Remove the right side I/P lower closeout, hush panel, retainers.
5. Pull the closeout panel, hush panel, rearward to detach from the forward retainers.
6. Remove the right side heater outlet assembly retainer and remove the outlet.
7. Remove the glove compartment fasteners and the door.
8. Remove the glove compartment bin fasteners.
9. Slowly remove the glove compartment bin and tilt the bin downward to expose the BCM residing on top of the glove compartment.
10. Remove the BCM from the glove compartment by sliding the module out of the attaching slots.
11. Remove the glove compartment bin.
12. Let the BCM hang on the wiring harness.
13. Remove the right hinge pillar molding, kick panel.

13.1. | Remove the upper push pin fastener using a trim panel tool.

13.2. | Remove the fuse box door and pull on the hinge pillar molding at the clip location to disengage the molding.

13.3. | Slide the hinge pillar molding out from under the carpet retainer and remove the hinge pillar molding.

14. Gain access to the rear of the radio and connect the CD I/P harness to the radio.

Important: The I/P harness connector, the antenna connector, and the ground strap terminal do not need to be disconnected, unless the radio needs to be upgraded. Ensure connection.

14.1. | Remove the radio. Refer to Radio Replacement .

14.2. | Upgrade the radio, if necessary, to AM/FM stereo cassette player and CD player with equalizer, UP0.

14.3. | Connect the I/P CD jumper connector to the rear of the radio.

| Important: Do not secure the radio or trim in place until the CD changer/player is installed and verified to be functioning correctly.

14.4. | Set the radio into the radio brace.

15. Route the I/P CD jumper from the rear of the radio to right I/P fuse block.

15.1. | Route the I/P CD jumper behind the right side of the radio to the right of the H-brace, along side of the current routing for the I/P harness.

15.2. | Attach the I/P CD jumper to the I/P lead that connects to the radio using the buddy clip on the harness to hold the jumper in place.

15.3. | Route the I/P CD jumper along the I/P beam and attach the fir tree clips to the vertical side of the beam forward in the car. These clips are located just below the current routing for the I/P harness in the area above the glove compartment bin.

15.4. | Route the I/P CD jumper the rest of the way to the right I/P fuse block area.

### Body CD Jumper Installation

1. Remove the right side carpet retainer, sill plate.

1.1. | Move the front seat to a forward most position.

1.2. | Starting at the front of the vehicle, remove the carpet retainer by gently pulling on the retainer at the attaching clip locations.

2. If leather seats, move rear seat cushion forward before removing bolster to avoid damage to leather.

If the seat is not leather, movement is not necessary.

3. Remove the right rear seat bolster.

• | Reach down into the outer corner of rear seat cushion to expose the bolster retainer tab.

• | Bend the tab upward.

• | Starting at the bottom, pull forward to disengage bolster from retainer tab, then pull upward to disengage upper attachment.

4. Remove the cargo shade.
5. Lower the rear seat back assembly.
6. Gently pull at the attaching clip locations and remove the cargo shade side molding.
7. Remove the rear load floor.

7.1. | Flip the load side-wing(s) upwards.

7.2. | Lift the load floor upwards.

7.3. | Slide the load floor tabs out of the front load floor assembly.

7.4. | Lift the load floor out of the vehicle.

8. Remove the cargo net fasteners.
9. Gently pull at clip locations and remove rear cargo area side carpet.
10. Route the body CD jumper along the right side of vehicle starting at area between rear seat and rear cargo area.
11. Route the body CD jumper around the rear seat support bracket and put enough of the harness through to reach the CD changer/player location.

Notice: Make sure the body CD jumper is lined up correctly with holes before attaching them. The clips are easily damaged when removed.

12. Install the body CD jumper to the vehicle starting with the jumper clip nearest the CD changer/player connector. Attach all of the other clips as you route the body CD jumper to rear seat area.
13. Route the body CD jumper along the rear seat and install the jumper to the vehicle using the attachment clips.
14. Open the harness channel found in the right inner rocker panel area and install the body CD jumper.
15. After installing the harness, close the harness channel.
16. Connect the body CD jumper connector to I/P CD jumper connector which was routed earlier and is located near the right I/P fuse block (RIPFB) area.
17. Connect the body CD jumper connector to RIPFB using the rosebud clip on the connector.

### CD Changer/Player Installation

1. Place the CD changer/player into the CD changer/player compartment.

Notice: Refer to Fastener Notice in the Preface section.

Important: Do not substitute the type of fastener that attaches the CD changer/player to CD changer/player compartment. Otherwise, shock dampening mechanism will be disabled.

2. Line up the holes in the CD changer/player with the CD changer/player compartment and install the fasteners.

Tighten
Tighten the CD changer/player-to-CD changer/player compartment fasteners to 4 N·m (35 lb in).

3. Install the U-nuts to the sheet metal.
4. Using a sharp knife, carefully cut a hole in the rear cargo area side carpeting as indicated in illustration for connector to go through.
5. Pull the connector and harness through as far as possible.
6. Install the rear cargo area side carpeting to the vehicle with integral clips making sure carpet is slid under liftgate lower molding.
7. Install the cargo net fasteners.

Tighten
Tighten the cargo net fasteners to 2.5 N·m (22 lb in).

8. Using the CD changer/player compartment as a template, mark with a pen or sharp tool where mounting holes should go through carpet.
9. Pull the CD changer/player compartment away and carefully cut holes using a sharp knife.
10. Make electrical connection and temporarily connect the negative battery cable. Verify that CD changer/player is functioning properly, then disconnect the negative battery cable.
11. Install the CD changer/player compartment into the vehicle by first attaching the compartment to the side of the vehicle then attaching it to floor of vehicle.

Tighten
Tighten the CD changer/player compartment-to-vehicle fasteners to 8 N·m (71 lb in).

### Removed Parts From Harness Installation

Important: Ensure that the I/P harness connector, antenna connector, and the ground strap connector are connected.

1. Install the radio. Refer to Radio Replacement .
2. Install the glove compartment bin partially into the opening.
3. Secure the BCM to the glove compartment bin slots.
4. Route the glove compartment lamp wiring harness to the lamp opening and connect the wiring harness to the glove compartment lamp.
5. Snap the lamp into the glove compartment bin.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the glove compartment bin to I/P fasteners.

Tighten
Tighten the glove compartment bin-to-I/P fasteners to 2.5 N·m (22 lb in).

7. Install the heater outlet with the retainer to glove compartment bin.
8. Install the right lower I/P closeout panel, hush panel, with retainers.
9. Install the glove compartment door with fasteners.

Tighten
Tighten the glove compartment door fasteners to 2 N·m (18 lb in).

10. Operate the glove compartment lamp and glove compartment door to assure proper operation.
11. Install the right hinge pillar molding, kick panel.

11.1. | Side the hinge pillar molding into the carpet retainer.

11.2. | Position the hinge pillar molding to body and install by pushing gently at clip location.

11.3. | Install the hinge pillar molding upper push pin fastener.

11.4. | Install the fuse box door.

11.5. | Install the weather-strip over the hinge pillar molding cover using a flat blade tool.

12. Install the right side carpet retainer, sill plate.

12.1. | Position the carpet retainer into the vehicle.

12.2. | Starting at the rear of the vehicle, slide the carpet retainer under the rear seat cushion.

12.3. | Position the carpet retainer over the remaining attaching clip locations.

12.4. | Gently push on the attaching clips to install the carpet retainer.

12.5. | Install the weather-strip over the carpet retainer using a flat blade tool.

Important: If leather rear seat cushion was removed, install it after installing right rear seat bolster.

13. Install the right rear seat cushion bolster.

13.1. | Position the rear seat bolster onto the upper bolster attachment.

13.2. | Push down on the bolster to engage upper attachment and install over retaining tab.

13.3. | Bend the lower retainer tab over the bolster wire frame at the rear seat cushion location.

14. Install the rear load floor.

14.1. | Drill the load floor right side-wing rivets out and remove the right side-wing.

14.2. | Flip the left side-wing (if present) upwards.

14.3. | Place the load floor into the vehicle.

14.4. | Lift the load floor upwards.

14.5. | Slide the load floor tabs into the front load floor assembly.

15. Install the cargo shade side molding by pushing at clip locations.
16. Install the rear cargo shade.
17. Raise the rear seat back assembly.
18. Install the liftgate weather-strip over the side carpet using a flat blade tool.

### Remote CD Changer/Player Installation Finishing Touches

1. Enable the SIR System. Refer to Enabling the SIR System in SIR.
2. Connect the negative battery cable.
3. Test the operation of CD Changer/Player. If the CD Changer/Player does not operate correctly, refer to the troubleshooting portion of this audio section.
4. Set earlier recorded radio preset stations and clock time.
5. Remind customer that the Theft Deterrent Feature is not activated and that it needs to be reactivated if continued security is desired.