For 1990-2009 cars

### Removal Procedure

1. Remove the rear door window. Refer to Rear Side Door Window Replacement .
2. Disconnect the electrical connection, if equipped.
3. Remove the rear window regulator bolts.
4. Remove the rear door window regulator from the door.

### Installation Procedure

1. Install the rear door window regulator to the rear door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts to the rear door window regulator.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Connect the electrical connection, if equipped.
4. Install the rear door window. Refer to Rear Side Door Window Replacement .
5. Inspect the rear door window regulator for proper operation.