For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
2. Insert a flat-bladed tool between the instrument panel (I/P) and light sensor.
3. Carefully pry the sensor assembly from the I/P.
4. Disconnect the wire connector.

### Installation Procedure

1. Install the wire connector to the sensor.
2. Push in the sensor assembly until fully seated.
3. Install the instrument cluster trim bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .