For 1990-2009 cars

### Removal Procedure

1. Grab the trim plat at the A/C vent area and pull gently to disengage the attaching clips.
2. Tilt the trim plate sideways, disconnect the electrical harnesses and remove the trim plate.

### Installation Procedure

1. If the center trim plate is being replaced, transfer the center trim plate electrical switches to the new center trim plate.
2. Connect the electrical harnesses to the switches.
3. Snap the center trim plate into the I/P.