For 1990-2009 cars

### Removal Procedure

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
2. Remove the rear hood seal. Refer to Hood Rear Seal Replacement in Body front End.
3. Remove the air inlet grill.
4. Disconnect the electrical connector from the wiper motor.
5. Remove the bolts from the wiper motor.
6. Remove the wiper motor from the plenum area.
7. If replacing the wiper module bushings, remove the steel bushing first, then the rubber grommet.
8. Remove the wiper motor from the transmission.

### Installation Procedure

1. Install the wiper motor to the transmission.
2. If the wiper module bushings were replaced, install the rubber grommet first, then the steel bushing.
3. Install the wiper motor to the plenum area.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the wiper motor bolts.

Tighten
Tighten the bolts to 5 N·m (44 lb in).

5. Connect electrical connector to wiper motor.
6. Install the rear hood seal. Refer to Hood Rear Seal Replacement in Body front End.
7. Install air inlet grill. Refer to .
8. Install wiper arm. Refer to Windshield Wiper Arm Replacement .
9. Inspect the wiper/washer system for proper operation.