For 1990-2009 cars

## Door Lock Switch Replacement Front

### Removal Procedure

1. Using a small blade tool, gently pry on the switch to disengage the retainers.
2. Pull the switch away from the handle and disconnect the switch wiring harness.
3. Remove the switch.

### Installation Procedure

1. Connect the door lock switch wiring harness.
2. Snap the door lock switch into place.
3. Test the switch to ensure proper operation.