For 1990-2009 cars

### Removal Procedure

1. Remove the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement in Doors.

Important: Observe the wiring harness routing inside the door handle to aid in the installation.

2. Disconnect the tweeter speaker harness while holding the inner door handle away from the door trim panel.
3. Remove the tweeter speaker.

### Installation Procedure

1. Install the tweeter speaker to the inner door handle assembly.
2. Connect the tweeter speaker wiring harness to the tweeter speaker.
3. Install the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement in Doors.