For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Disconnect the electrical connector from the latch assembly.
3. Remove the screws from the latch assembly.
4. Unhook the lock cylinder actuator cable from the latch assembly.
5. Remove the latch assembly.

### Installation Procedure

1. Install the latch assembly.
2. Hook the lock cylinder actuator cable to the latch assembly.
3. Install the screws to the latch assembly.

Tighten
Tighten the decklid latch-to-decklid fasteners to 10 N·m (89 lb in).

4. Connect the electrical connector to the latch assembly.
5. Close the rear compartment lid.