For 1990-2009 cars

### Removal Procedure

1. Remove the lower dash closeout panel and the hush panel from the driver side.
2. Remove the lower air duct from the driver side.
3. Remove the gas pedal to provide access to the temperature actuator.
4. Remove the lower console closeout panel.
5. Remove the screws attaching the temperature door actuator.
6. Disconnect the electrical connection from the temperature door actuator.

### Installation Procedure

1. Connect the electrical connection to the temperature door actuator.
2. Install the temperature door actuator and the attaching screws.
3. Install the lower console closeout panel.
4. Install the gas pedal.
5. Install the lower air duct.
6. Install the lower dash closeout panel and the hush panel.