For 1990-2009 cars

#### Tools Required

• | J 23327 Clutch Spring Compressor

• | J 41232 Return Spring Compressor

1. In order to aid in the assembly, lubricate the seal with transmission fluid.
2. Assemble the 2nd clutch piston and seal assembly (404) into the driven sprocket support (401).
3. Assemble the 2nd clutch spring and retainer assembly (405) into the driven sprocket support.
4. Compress the 2nd clutch spring assembly. Use the J 41232 and J 23327 or equivalent.
5. Assemble the 2nd clutch spring retainer snap ring (406).
6. Remove the J 41232 and J 23327 .
7. Assemble two new seal rings (403) onto the driven sprocket support.