For 1990-2009 cars

Notice: Front cover damage and engine damage will result if thegerotor gears are not properly installed into the front cover.

1. Install the gear with the groove in the gear aligning with the race in the front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the gerotor cover and bolts.

Tighten
Tighten the oil pump geroter cover bolts to 6 N·m (53 lb in).

3. Install the pressure relief valve piston.
4. Install the pressure relief valve spring.
5. Install the pressure relief valve plug.

Tighten
Tighten the oil pump pressure relief valve plug to 40 N·m (30 lb ft).