For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable-to-Battery | 17 N·m | 13 lb ft
Battery Feed-to-Fuse Block | 16 N·m | 12 lb ft
Battery Hold Down | 20 N·m | 15 lb ft
Battery Tray Bolts | 15 N·m | 11 lb ft
Cooling Fan-to-Radiator Bolts | 4 N·m | 35 lb in
Exhaust Manifold Pipe Heat Shield Bolts (L81) | 8 N·m | 71 lb in
Front Transaxle Mount Through Bolt | 55 N·m | 41 lb ft
Front Transaxle Mount-to-Transaxle Bolts | 90 N·m | 66 lb ft
Fuse Block-to-Battery Tray Bolts | 9 N·m | 80 lb in
Left Transaxle Mount Bracket-to-Transaxle Bolts - Automatic | 90 N·m | 66 lb ft
Left Transaxle Mount Bracket-to-Transaxle Bolts - Manual | 55 N·m | 41 lb ft
Left Transaxle Mount Bracket-to-Transaxle Mount Bolt | 60 N·m | 44 lb ft
Left Transaxle Mount-to-Body Bolts | 20 N·m | 15 lb ft
Left Transaxle Mount-Transaxle Bracket Bolts | 55 N·m | 41 lb ft
Power Steering Lines-to-Transaxle Mount Bracket | 10 N·m | 89 lb in
Rear Transaxle Mount Bracket-to-Frame Bolts | 60 N·m | 44 lb ft
Rear Transaxle Mount Bracket-to-Transaxle Bolts | 90 N·m | 66 lb ft
Rear Transaxle Mount Through Bolt | 90 N·m | 66 lb ft
Rear Transaxle Mount-to-Frame Bolts | 60 N·m | 44 lb ft
Rear Transaxle Mount-to-Transaxle Bolts | 90 N·m | 66 lb ft
Right Engine Mount Bracket-to-Engine Bolts (L61) | 90 N·m | 66 lb ft
Right Engine Mount Bracket-to-Engine Bolts (L81) | 55 N·m | 41 lb ft
Right Engine Mount Bracket-to-Engine Mount | 90 N·m | 66 lb ft
Right Engine Mount-to-Body Bolts | 55 N·m | 41 lb ft
Axle Shaft-to-Hub

- Initial Torque

100-160 N·m

74-118 lb ft

- Final Torque

20 N·m + 90 degrees

15 lb ft + 90 degrees

Lower Control Arm-to-Steering Knuckle | 100 N·m | 75 lb ft
Tie Rod End Linkage Installer | 45 N·m | 33 lb ft
Tie Rod End-to-Steering Knuckle Nut | 60 N·m | 44 lb ft
Wheel Bolts

- Initial Torque

63 N·m

46 lb ft

- Final Torque

125 N·m

92 lb ft

Right Engine Mount-to-Bracket Bolts | 55 N·m | 41 lb ft