For 1990-2009 cars

## Radio Rear Side Door Speaker Replacement Tweeter

### Removal Procedure

1. Remove the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement in Doors.

Important: Observe the wiring harness routing inside the door handle to aid in the installation.

2. Disconnect the tweeter speaker harness while holding the inner door handle away from the door trim panel.
3. Remove the tweeter speaker.

### Installation Procedure

1. Install the tweeter speaker to the inner door handle assembly.
2. Connect the tweeter speaker wiring harness to the tweeter speaker.
3. Install the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement in Doors.

## Radio Rear Side Door Speaker Replacement Woofer

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the speaker fasteners and pull the speaker away from the door assembly.
3. Disconnect the electrical connector from the speaker.
4. Remove the speaker from the vehicle.

### Installation Procedure

1. Connect the speaker electrical connector to the speaker.
2. Position the speaker in the door assembly, with the word TOP at the top of the speaker.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the fasteners.

Tighten
Tighten the fasteners to 1.5 N·m (13 lb in).

4. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .