For 1990-2009 cars

#### Tools Required

J 38122-A Harmonic Balancer Holder

1. Install the J 38122-A .
2. Remove the damper retaining bolt and washer. Use the J 38122-A and a breaker bar in order to prevent the crankshaft from rotating when loosening the bolt.

Discard the bolt.

3. Remove the damper assembly.

#### Tools Required

J 38122-A Crankshaft Pulley Holder

### Removal Procedure

1. Install the J 38122-A onto the damper assembly.
2. Remove and discard the damper retaining bolt and washer. Use the J 38122-A and breaker bar in order to prevent the crankshaft from rotating when loosening the bolt.
3. Remove the damper assembly.