For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antilock Brake System (ABS) Sensor Bracket-to-Knuckle | 8 N·m | 71 lb in
ABS Sensor-to-Bracket | 4 N·m | 35 lb in
Caliper Mount Bracket-to-Knuckle | 95 N·m | 70 lb ft
Control Arm-to-Frame | 90 N·m + 75-90 degrees | 66 lb ft + 75-90 degrees
Exhaust Manifold Pipe Heat Shield Bolts (L81) | 8 N·m | 71 lb in
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 30 N·m | 22 lb ft
Exhaust Manifold Pipe-to-Exhaust Pipe Bolts | 20 N·m | 15 lb ft
Exhaust Manifold Pipe-to-Pipe Bolts | 20 N·m | 15 lb ft
Exhaust Manifold Pipe-to-Resonator Bolts | 20 N·m | 15 lb ft
Frame Assembly-to-Body Bolts | 90 N·m + 45-60 degrees | 66 lb ft + 45-60 degrees
Front Rotor-to-Hub | 3.5 N·m | 27 lb in
Front Strut-to-Body Upper Nut | 55 N·m | 41 lb ft
Front Strut-to-Knuckle

- Initial Torque

50 N·m

37 lb ft

- Final Torque

100 N·m + 30-45 degrees

73 lb ft + 30-45 degrees

Front Transaxle Mount Through Bolt | 55 N·m | 41 lb ft
Lower Control Arm-to-Steering Knuckle | 100 N·m | 74 lb ft
O2 Sensor Clip-to-Underbody Attachment Nut | 4 N·m | 35 lb in
Rear Transaxle Mount Through Bolt | 90 N·m | 66 lb ft
Rear Transaxle Mount-to-Frame Bolts | 60 N·m | 44 lb ft
Right Splash Shield-to-Body | 5 N·m | 44 lb in
Spring Seat Nut-to-Front Strut Shaft | 55 N·m | 40 lb ft
Stabilizer Bar Clamp-to-Frame Bolts | 20 N·m | 15 lb ft
Stabilizer Bar Link-to Strut | 65 N·m | 48 lb ft
Stabilizer Bar-to-Stabilizer Bar Link | 65 N·m | 48 lb ft
Steering Gear Heat Shield-to-Frame | 4 N·m | 35 lb in
Steering Gear-to-Frame | 45 N·m + 90 degrees | 35 lb ft + 90 degrees
Suspension Support-to-Body Bolts | 90 N·m + 45-60 degrees | 66 lb ft + 45-60 degrees
Tie Rod End Linkage Installer | 45 N·m | 33 lb ft
Tie Rod End-to-Knuckle Nut | 60 N·m | 45 lb ft
Wheel Bolts

- Initial Torque

63 N·m

46 lb ft

- Final Torque

125 N·m

92 lb ft