For 1990-2009 cars

| Specifications
--- | ---
Application | Metric | English
Accelerator Pedal Position Assembly-to-Brake Bracket Bolt | 25 N·m | 18 lb ft
Battery Terminal Bolts | 17 N·m | 13 lb ft
Belt Tensioner Bolts | 40 N·m | 30 lb ft
Camshaft Position Sensor | 8 N·m | 71 lb in
Crankshaft Position Sensor Bolt | 8 N·m | 71 lb in
Engine Control Module Attachment Bolts | 8 N·m | 71 lb in
Engine Coolant Temperature Sensor | 18 N·m | 13 lb ft
Engine Oil Pressure Switch | 10 N·m | 89 lb in
Generator Mounting Bolts | 40 N·m | 30 lb ft
Ignition Module Bolts | 8 N·m | 71 lb in
Intake Plenum Switchover Valve Bolts | 8 N·m | 71 lb in
Knock Sensor Bolt | 20 N·m | 15 lb ft
Manifold Absolute Pressure Sensor Bolt | 5 N·m | 44 lb in
Oxygen Sensors (Exhaust Manifold) | 50 N·m | 37 lb ft
Oxygen Sensors (Lower Exhaust Pipe) | 45 N·m | 33 lb ft
Power Steering Pump Pulley Bolt | 20 N·m | 15 lb ft