For 1990-2009 cars

### Removal Procedure

1. Operate the sunroof to the ¼ open position.
2. Remove the 4 screws from the "U" cover.
3. Close the sunroof and put in the vent position.
4. Remove the "U" cover by un-snapping the sides and the lower cover down into the passenger compartment.
5. Remove the 4 bolts from the encapsulated glass.
6. Remove the water channel screws (2).
7. Slide the sunshade forward.
8. Remove the sunshade from the above vehicle by pressing the sunshade guide clips.
9. If the sunshade clips are to be replaced, remove the sunshade guide clips by using a small screwdriver to bend the retaining tangs up.

### Installation Procedure

1. If the sunshade guide clips were replaced, install the sunshade guide clips by pressing the clips onto the sunshade where the old clips were located.
2. Install the sunshade from above the vehicle by installing the 2 sunshade guide clips.
3. Slightly tilting one side of the sunshade more forward than the other side, install the remaining 2 guide clips by pressing the guide clip and pushing into the channel. This will help to engage the clips into the channel.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the water channel screws. Tighten the driver side screw first and the passenger side screw in the second slot.

Tighten
Tighten the water channel screws to 3 N·m (27 lb in).

5. Install the encapsulated glass with the 4 bolts. Do not tighten at this point.
6. Align the encapsulated glass to the roof in the 4 locations as indicated by the arrows, 0-1 mm (0-3/64 in) lower than the roof in the front and 0-1 mm (0-3/64 in) higher than the roof in the rear.
7. Tighten the encapsulated bolts.

Tighten
Tighten the encapsulated glass-to-sunroof module fasteners to 4 N·m (35 lb in).

8. Install the "U" cover by snapping the sides to the sunroof assembly.
9. Operate the sunroof to the ¼ open position.
10. Install the 4 screws to the "U" cover.

Tighten
Tighten the sunroof module "U" cover retaining screws to 4 N·m (35 lb in).

11. Verify a smooth operation.
12. Verify the alignment to the roof.
13. Adjust by loosening the bolts, repositioning the glass, and retightening in a new position.