For 1990-2009 cars

### Removal Procedure

1. Remove the door lock switch. Refer to Door Lock Switch Replacement .
2. Remove the power mirror switch on the driver side door. Refer to Power Mirror Switch Replacement .
3. Using a small flat-bladed tool, remove the tweeter cover.
4. Remove the upper door trim panel. Refer to Upper Extension Trim Panel Replacement .
5. Remove the fastener cover from the inner pull handle.
6. Remove the fasteners.
7. Remove the pull handle.

### Installation Procedure

1. Install the pull handle to the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fasteners to the pull handle.

Tighten
Tighten the fasteners to 2 N·m (17.7 lb in).

3. Install the cover to the fasteners.
4. Install the upper door trim panel. Refer to Upper Extension Trim Panel Replacement .
5. Install the tweeter cover.
6. Install the power mirror switch on the driver side door. Refer to Power Mirror Switch Replacement .
7. Install the door lock switch. Refer to Door Lock Switch Replacement .