For 1990-2009 cars

### Removal Procedure

1. Using a flat-bladed tool, pry on the switch to disengage the clips.
2. Remove the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement .
3. Remove the cover from the pull handle electrical connector.
4. Disconnect the pull handle electrical connector.
5. Remove the door lock switch from the pull handle.

### Installation Procedure

1. Install the door lock switch to the pull handle.
2. Connect the electrical connector to the pull handle.
3. Install the cover to the electrical connector.
4. Install the rear door pull handle. Refer to Rear Side Door Pull Handle Replacement .
5. Snap the switch onto the pull handle.