For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
B+ Cable-to-Generator Nut | 16 N·m | 12 lb ft
B+ Cable-to-Starter Nut | 9 N·m | 80 lb in
Battery Hold-Down Bracket | 20 N·m | 15 lb ft
Battery Hold Down Bracket Bolt | 20 N·m | 15 lb ft
Battery Terminal Bolts | 17 N·m | 13 lb ft
Battery Tray Fasteners | 15 N·m | 11 lb ft
Belt Tensioner Bolts | 40 N·m | 30 lb ft
Generator Mounting Bolts | 40 N·m | 30 lb ft
Generator-to-Engine Block Bolts | 20 N·m | 15 lb ft
Ignition Switch Module Screws | 1.5 N·m | 13.3 lb in
Starter-to-Engine Bolts (L81) | 40 N·m | 30 lb ft
Negative Battery Cable to Chassis | 12.5 N·m | 9.5 lb ft
Positive Battery Cable-to-Generator Nut | 16 N·m | 12 lb ft
Positive Battery Cable-to-Starter Nut | 9 N·m | 80 lb in
S-Terminal Nut | 4.5 N·m | 40 lb in
S-Terminal Wire-to-Starter Nut | 4.5 N·m | 40 lb in
Starter-to-Engine Bolts (L61) | 40 N·m | 30 lb ft
Transaxle Range Switch Bolts | 20 N·m | 15 lb ft
Transaxle Range Switch Lever Nut | 35 N·m | 26 lb ft
Upper Starter Mounting Bolts | 40 N·m | 30 lb ft
Wheel Bolts (Final Torque) | 125 N·m | 92 lb ft
Wheel Bolts (Initial Torque) | 63 N·m | 46 lb ft