For 1990-2009 cars

## Rear Side Door Window Weatherstrip Replacement New Style

### Removal Procedure

Important: The old 1-piece weatherstrip design will work in place of the new 2-piece design.

1. Lower the rear door window.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Verify if the front weatherstrip guide and weatherstrip is a 1-piece weatherstrip or the new 2-piece design.
5. Remove the bolt from the weatherstrip guide .
6. Remove the weatherstrip guide pressing down and out of the door.
7. Remove the weatherstrip from the door.

### Installation Procedure

1. Install the weatherstrip guide to the door by pushing the clip on the guide up into the down slot.
2. Install the weatherstrip to the door.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the weatherstrip guide bolt.

Tighten
Tighten the bolt to 10 (89 lb in).

4. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
5. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
6. Inspect the rear door window for proper alignment and operation.

## Rear Side Door Window Weatherstrip Replacement Old Style

### Removal Procedure

Important: The old 1-piece weatherstrip design can not be serviced with the new 2-piece design without using the new window with the concave front edge.

1. Lower the rear door window.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Remove the weatherstrip from the weatherstrip guide.
5. Remove the bolt from the weatherstrip guide.
6. Remove the weatherstrip guide from the door.
7. Remove the weatherstrip by lifting up and out of the door.

### Installation Procedure

1. Install the weatherstrip to the window run channel by sliding down and into the run channel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the weatherstrip guide to the door by pushing the clip on the guide up into the down slot.
3. Install the weatherstrip guide bolt.

Tighten
Tighten the bolt to 10 (89 lb in).

4. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
5. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
6. Inspect the rear door window for proper alignment and operation.