For 1990-2009 cars

Symptom | Procedure
--- | ---
All windows inoperative from all switches. | Chart 1
Both left windows inoperable or both right windows inoperable. | Chart 2
Only left front or only right front window inoperable. | Chart 3
Left rear or right rear window inoperable from both the master window switch in the console and from the rear door window switch. | Chart 4
Left rear or right rear window inoperable from its rear door window. | Chart 5
Left rear or right rear window inoperable from only the master window switch in the console. | Chart 6
Both left rear and right rear windows inoperable from rear door window switches. |

• | Verify that the rear window lockout switch is in the ON position.

• | If the rear doors won't function when the rear window lockout switch is in the ON position, replace the Left Master Window Switch in the console.

• | Check power window operation from all window switches.

Rear window lockout switch does not lockout the rear door window switches. |

• | Verify that the rear window lockout switch is in the OFF position.

• | If the rear doors still function in the OFF position, replace the Left Master Window Switch in the console.

• | Check power window operation from all window switches.

Front window auto down inoperable. |

• | Verify that the auto down feature is inoperable.

• | Replace Left Master Window Switch in the console.

• | Check motor and replace if necessary.

• | Check for mechanical/binding problems and fix if necessary.

• | Check power window operation from all window switches.

A window won't go down all the way. |

• | Check for mechanical/binding problem and fix if necessary.

• | Check ground (BLK circuit 450) between Master Console Switch (terminal F for left master switch or terminal B for right master switch) and a known good ground.

• | Check motor and replace if necessary.

• | Check power window operation from all window switches.

### All Windows Inoperative From All Switches - Chart 1

### Both Left Windows Inoperable or Both Right Windows Inoperable - Chart 2

### Only Left Front or Only Right Front Window Inoperable - Chart 3

### Left Rear or Right Rear Window Inoperable From Both the Master Window Switch in the Console and From the Rear Door Window Switch - Chart 4

### Left Rear or Right Rear Window Inoperable From Rear Door Window Switch Only - Chart 5

### Left Rear or Right Rear Window Inoperable From Only the Master Window Switch in the Console - Chart 6