For 1990-2009 cars

### Removal Procedure

1. Remove the engine cooling fan attachment bolts.

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

2. Raise the vehicle.
3. Position the engine cooling fan to allow access to the transaxle mount bolts.
4. Remove the front transaxle mount through bolt.
5. Remove the transaxle mount-to-transaxle attachment bolts.
6. Remove the transaxle mount from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle mount into the vehicle and tighten the bolts.

Tighten
Tighten the transaxle mounts (front and rear)-to-transaxle bolts to 90 N·m (66 lb ft).

2. Install the transaxle mount through bolt.

Tighten
Tighten the transaxle mount (rear) through bolt to 55 N·m (41 lb ft).

3. Reposition the cooling fan for installation.
4. Lower the vehicle from the hoist.
5. Install the engine cooling fan attachment bolts.

Tighten
Tighten the engine cooling fan attachment bolts to 4 N·m (35 lb in).